A 96 channels, 500

A 96 channels, 500 psps resolution TDC board for the resolution TDC board for the BABARAR experiment at SLAC experiment at SLAC

S. Minutoli^1 and E. Robutti^{1,2}

1Istituto Nazionale di Fisica Nucleare, Sezione di Genova, 16146 Genova, Italy 2Universit� degli Studi di Genova, Dipartimento di Fisica, 16146 Genova, Italy

Abstract

A TDC board has been designed and built to complete the readout of the Instrumented Flux Return of the BaBar experiment at the Stanford Linear Accelerator Center. The board has 96 input channels and makes use of 3 multi-purpose TDC chips designed at CERN, with time resolution up to 500�ps and configurable via a Test Access Port (IEEE standard 1149). Data are stored before readout in a multi-event buffer. Communication with BaBar DAQ system is realized through 3 serial lines on the backplane connector. All the logic, including internal registers and the interfaces with the BaBar protocol and the TAP controller, is implemented in two fast FPGAs. The board is designed to work at 59.5 MHz clock frequency.

Simplified block diagram of the ITB

Block diagram of the 32-channel CERN chip

Instrumented Flux Return

ITB Time Distribution (all 96 channels)

T (clock ticks) 0

100

200

300

400

500

600

0 25 50 75 100 125 150 175 200 225 250

ITB time distribution for a BaBar cosmic rays run. The peak width is mainly due to the jitter of BaBar trigger.

Specifications

Input Signals ECL diff. (96 channels)

Operating Clock Frequency

59.5 MHz

Time Bin Size 525 ps (= T/32)

Dynamic Range 21 bit (1.1 ms)

Data Bus 32 lines

Event Buffer Size 512 × 32 (> 5 full sized events)

Communication BABAR protocol (3 serial lines) on custom VME-like backplane

Maximum Trigger/Readout Rate (for full sized events)

58.5 kHz

Registers 3 configuration (128 × 1), 3 mask (32 × 1), 3 error (32 × 1)

Configurability �trigger matching� window offset and width; trigger time subtraction flag; global offset; single channels offset; channel masks.

Block diagram of the ITB Command Decoder / Registers / TAP Interface logic (XC4006E-1)

The

Instrumented

FluxReturn (

IFR) is one of the 5 major subdetectors building up the BaBar apparatus on the PEPII e^+e^− collider at SLAC. Its active part is made up of Resistive Plate Chambers (RPCs), whose signals are read out by means of ~50,000 aluminum strips. Timing of these signals is useful for prompt bunch crossing determination, pattern recognition and noise rejection. The ITB (IFR TDC Board) has been developed for this purpose and is part of the IFR frontend electronics; this is installed right outside the detector and is connected via a 1GHz optical link to the DAQ system inside the BaBar electronics house. To serve its purpose, the ITB has to fullfill several requirements: - it must have good time resolution, at least as good as the intrinsic RPC resolution of ~1�ns. This is necessary to deal with the close spacing of PEPII bunch crossings (4.2�ns). - it has to comply fully with BaBar data transmission protocol, which makes use of 3 serial lines (a 59.5 MHz clock line, a command/data-in line and a data-out line) and a set of commands with related timing specifications. - it must be able to work in the same VME-like crate as the other IFR front-end boards,, sharing the same custom backplane (PDB).

Main components

TDC: CERN 32 channel multi-purpose TDC - Clock frequency: 20 MHz to 60 MHz - Time bin / dynamic range: 0.52�ns at 60 MHz / 21 bit - Highly configurable via JTAG Test Access Port Logic: Xilinx XC4006E-1 and XC3142A-1 - Ultra-high speed FPGAs - Number of logic cells: 256 (XC4006), 144 (XC3142) - On-chip synchronous RAM (XC4006)

Event Buffer: Texas Instruments SN74ACT3631-15 - 512�×�36 clocked dual port FIFO memory - Clock frequency: up to 67�MHz - Independent clock for the two R/W ports